
|  |  |
| --- | --- |
| **Description** | **Part Code** |
| Signaline FT-78-EN Non-resettable linear heat detector 78 deg C | SL-FT-78-EN |
| Signaline FT-78-EN Non-resettable linear heat detector 88 deg C | SL-FT-88-EN |
| Signaline Locator Plus-EN alarm location and interface module | SLP-002 |
| Signaline FT-EOL-EN two zone end of line with test switches | FT-EOL-EN |
| P Clip - Stainless Steel Clip with Insulator (pack of 100) | SL-FX/P |
| P Clip - Stainless Steel Clip with Insulator (pack of 25) | SL-FX/P/25 |





A picture containing text, clipart

Description automatically generatedText, logo

Description automatically generatedText, logo

Description automatically generatedA picture containing text, clipart

Description automatically generated

A picture containing text, clipart

Description automatically generatedText, logo

Description automatically generated­­